|  |
| --- |
|  |
| |  |  | | --- | --- | | **UT207** | **Digital Clamp Multimeters** | | |  |  | | --- | --- | |  | http://www.uni-trend.com/Images/ZXWIT/UT207_W.jpg | |  |  | |  |  | | **SPECIFICATIONS**   |  |  |  | | --- | --- | --- | | **Basic Functions** | **Range** | **Best Accuracy** | | **DC Voltage** | 6.6V/66V/600V | http://www.uni-trend.com/Images/PLUSMN.GIF(0.8%+1) | | **AC Voltage** | 6.6V/66V/600V | http://www.uni-trend.com/Images/PLUSMN.GIF(1.2%+5) | | **DC Current** | 66A/1000A | http://www.uni-trend.com/Images/PLUSMN.GIF(1.5%+8) | | **AC Current** | 66A/1000A | http://www.uni-trend.com/Images/PLUSMN.GIF(2%+8) | | **Resistance** | 660/6.6k/66k/660k/ 6.6M/66M | http://www.uni-trend.com/Images/PLUSMN.GIF(1%+2) | | **Temperature** | -40°C~1000°C -40°F~1832°F |  | | **Frequency** | 660Hz/6.6kHz/66kHz/660kHz/ 6.6MHz/66MHz | http://www.uni-trend.com/Images/PLUSMN.GIF(0.1%+3) | | **Duty Cycle** | 0.1% ~ 99.9% | http://www.uni-trend.com/Images/TICK.GIF | | **Special Functions** |  |  | | **Auto Ranging** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Diode** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Continuity Buzzer** |  | http://www.uni-trend.com/Images/TICK.GIF | | **True RMS** | AC Voltage | **http://www.uni-trend.com/Images/TICK.GIF** | | **Surge Current** | AC Current | http://www.uni-trend.com/Images/TICK.GIF | | **Max/Min Mode** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Data Hold** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Sleep Mode** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Display Backlight** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Full Icon Display** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Low Battery Display** |  | http://www.uni-trend.com/Images/TICK.GIF | | **Input Impedance for AC Voltage Measurement** | Around 10M | http://www.uni-trend.com/Images/TICK.GIF | | **Max. Display** | 6666 | http://www.uni-trend.com/Images/TICK.GIF |   **GENERAL CHARACTERISTICS**   |  |  | | --- | --- | | **Power** | 9V Alkaline Battery (1604A or 6LF22) | | **LCD Size** | 47 x 30mm | | **Product Color** | Red and Grey | | **Product Net Weight** | 533g | | **Product Size** | 286 x 105 x 45mm | | **Standard Accessories** | Test Lead, Alkaline Battery, English Manual, Tool Box | | **Standard Individual Packingt** | Gift Box | | **Standard Carton Gross Weight** | 5pcs | | Standard Carton Gross Weight | 480 x 372 x 315mm (0.056 CBM Per Standard Carton) | | **Standard Carton Gross Weight** | 11kg |  |  |  | | --- | --- | | \*Available at Extra Cost Specifications and other information are subject to change without further notice. |  | | |  | |