|  |
| --- |
|    |
|

|  |  |
| --- | --- |
| **UT207** | **Digital Clamp Multimeters** |
|

|  |  |
| --- | --- |
|  | http://www.uni-trend.com/Images/ZXWIT/UT207_W.jpg |
|  |  |
|  |  |

 | **SPECIFICATIONS**

|  |  |  |
| --- | --- | --- |
| **Basic Functions** | **Range** | **Best Accuracy** |
| **DC Voltage** | 6.6V/66V/600V | http://www.uni-trend.com/Images/PLUSMN.GIF(0.8%+1) |
| **AC Voltage** | 6.6V/66V/600V | http://www.uni-trend.com/Images/PLUSMN.GIF(1.2%+5) |
| **DC Current** | 66A/1000A | http://www.uni-trend.com/Images/PLUSMN.GIF(1.5%+8) |
| **AC Current** | 66A/1000A | http://www.uni-trend.com/Images/PLUSMN.GIF(2%+8)  |
| **Resistance** | 660/6.6k/66k/660k/6.6M/66M | http://www.uni-trend.com/Images/PLUSMN.GIF(1%+2) |
| **Temperature** | -40°C~1000°C-40°F~1832°F |         |
| **Frequency** | 660Hz/6.6kHz/66kHz/660kHz/6.6MHz/66MHz | http://www.uni-trend.com/Images/PLUSMN.GIF(0.1%+3) |
| **Duty Cycle** | 0.1% ~ 99.9% | http://www.uni-trend.com/Images/TICK.GIF |
| **Special Functions** |   |   |
| **Auto Ranging**  |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Diode**  |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Continuity Buzzer**  |         | http://www.uni-trend.com/Images/TICK.GIF |
| **True RMS**  | AC Voltage | **http://www.uni-trend.com/Images/TICK.GIF** |
| **Surge Current**  | AC Current | http://www.uni-trend.com/Images/TICK.GIF |
| **Max/Min Mode** |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Data Hold** |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Sleep Mode** |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Display Backlight**  |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Full Icon Display** |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Low Battery Display** |         | http://www.uni-trend.com/Images/TICK.GIF |
| **Input Impedance for AC Voltage Measurement** | Around 10M   | http://www.uni-trend.com/Images/TICK.GIF |
| **Max. Display**  | 6666 | http://www.uni-trend.com/Images/TICK.GIF |

**GENERAL CHARACTERISTICS**

|  |  |
| --- | --- |
| **Power** | 9V Alkaline Battery (1604A or 6LF22) |
| **LCD Size** | 47 x 30mm |
| **Product Color** | Red and Grey |
| **Product Net Weight**  | 533g |
| **Product Size** | 286 x 105 x 45mm |
| **Standard Accessories**  | Test Lead, Alkaline Battery, English Manual, Tool Box |
| **Standard Individual Packingt** | Gift Box |
| **Standard Carton Gross Weight** | 5pcs |
| Standard Carton Gross Weight | 480 x 372 x 315mm (0.056 CBM Per Standard Carton) |
| **Standard Carton Gross Weight** | 11kg |

|  |  |
| --- | --- |
| \*Available at Extra CostSpecifications and other information are subject to change without further notice. |  |

  |
|  |

 |